
Made with NTRK Wizard 0.5


Parameters with !!! need to be revised when I finish other FMs


Current modified FMs
______________________________________________________________________________________________________________

IJA-IJN

+A6m2-11,-21, N : Cy0_0/!!!_1, squares, arm, CxMin0/1, Sakae 12, trim              OK clean 11,21,N
+A6m3-32  : Cy0_0/!!!_1, squares, arm, CxMin0/1, Sakae 21, trim                    OK clean
+A6m5a,b : Cy0_0/!!!_1, squares, arm, CxMin0/1, Sakae 21, trim                     OK clean a,b
+A6m5c : Cy0_0/!!!_1, squares, arm, CxMin0/1, Sakae 31, trim                       OK clean c
+A6m7-62,-63: Cy0_0/!!!_1, squares, arm, CxMin0/1, Sakae 31, Sakae 21, trim        OK clean

+B5N2 : Cy0_0/!!!_1, squares, arm, CxMin1, Sakae 11, trim                          OK clean 
+D3A1 : Cy0_0/!!!_1, squares, arm, CxMin0/1, Kinsei 44, trim                       OK clean
+G4M1  : Cy0_0/!!!_1, squares, arm, CxMin1, Kasei 11, trim                         OK clean

+H8K1 : Cy0_0

+Ki-21 I, II : Cy0_0

+Ki-27 : Cy0_0/!!!_1, squares, arm, PD-97, trim                                    OK clean

+Ki-43-I, -II : [-I] Cy0_0/!!!_1, Ha-25, CxMin0, CxMin1, squares, arm   [-II] Cy0_0/1, CxMin1, squares, arm, Ha-115-31, trim         OK clean

+Ki-45 Kai-Ko, Kai-Otsu, Kai-Hei, Kai-Tei : squares, arm, Cy0_0/!!!_1, Ha-102, trim    OK clean

+Ki-61-I Ko : squares, arm, Cy0_0/!!!_1, CxMin1, trim (!)top speed, Ha-40, trim      OK clean
+Ki-61-I Otsu : squares, arm, Cy0_0/!!!_1, CxMin1, trim                              OK clean
+Ki-61-I Hei : squares, arm, Cy0_0/!!!_1, CxMin1, trim                               OK clean

+Ki-84 : Cy0_0/!!!_1, CxMin1, squares, arm, CxMin1, Ha-45, trim                      OK clean

+Ki-100 : squares, arm, CxMin1, Cy0_0/!!!_1, trim, Ha-112-II, trim                   OK clean

+J2M3 : Cy0_0/!!!_1, squares, arm, CxMin1, Kasei 23, trim                            OK clean
+J2M5 : Cy0_0/!!!_1, squares, arm, CxMin1, Kasei 26a, trim                           OK clean

+N1K1Ja and b : Cy0_0/!!!_1, squares, arm, CxMin1, Homare 21, trim                   OK clean
+N1K2 : Cy0_0/!!!_1, squares, arm, CxMin1, Homare 21, trim                           OK clean
______________________________________________________________________________________________________________

USN


+F2A-1 : Cy0_0/!!!_1, squares, arm, CxMin1R-1820-G5, trim                                    OK clean
+F2A-2 : R-1820-40, VMax = 433 km/h, VMaxH= 500 km/h, Squares, Cy0_0/!!!_1, arm, trim        OK clean

+F4F-3,-4 : Cy0_0/!!!_1, squares, arm, CxMin1, R-1830-86, trim                               OK clean
+FM-2 : Cy0_0/!!!_1, squares, arm, CxMin1, R-1820-56W, trim                                   OK clean

+F6F-3,-5 : Cy0_0/!!!_1, squares, arm, CxMin1, R-2800-10,-10W, trim                          OK clean

+F4U-1,-1A,-1C,-1D : Cy0_0/!!!_1, squares, arm, CxMin1, R-2800-8,-8W, trim, !!!Reverts to 4.09 (AOACritH/L_0/_1)!!!, Empty weight    OK clean

+SBD-3 : Cy0_0/!!!1, CxMin0/1, R-1820-52, squares, arm, trim, Empty weight, Fuel, Oil, lvlstab  OK clean
+SBD-5 : Cy0_0/!!!1, CxMin0/1, R-1820-60, squares, arm, trim, Empty weight, Fuel, Oil, lvlstab  OK clean

+TBD-1 : Cy0_0                        OK clean
+TBF-1,1C,TBM-3 : Cy0_0               OK clean
______________________________________________________________________________________________________________

RN


+Corsair I, II, IV : Cy0_0/!!!_1, squares, arm, CxMin1, R-2800-8,-8W, trim, !!!Reverts to 4.09 (AOACritH/L_0/_1)!!!, Empty weight    OK clean

+Seafire F Mk.III : Merlin 55, Cy0_0/!!!1, CxMin1, squares, arm, trim                        OK clean
+Seafire L Mk.III : Merlin 55M, Cy0_0/!!!1, CxMin1, squares, arm, trim                       OK clean
______________________________________________________________________________________________________________

RAF


+Beaufighter Mk.21 : HerculesXVIII, !!Cy0_0/1!!, CxMin1, squares, arm, trim                      OK clean
+Beaufort Mk.I, early, late, Mk.II : Cy0_0                                                   OK clean
+Blenheim Mk.I, IV : Cy0_0!!!                                                                   OK clean

+Gladiator Mk.I/J8 :
+Gladiator Mk.II :

+Hurricane Mk.I : Merlin III 6 lb, Cy0_0/!!!1, CxMin0/1, squares, arm, trim                     OK clean
+Hurricane Mk.IIb : Merlin XX 12 lb, Cy0_0/!!!1, CxMin1, squares, arm, trim                     OK clean
+Hurricane Mk.IIc : Merlin XX 12 lb, Cy0_0/!!!1, CxMin1, squares, arm, trim                     OK clean
+Hurricane Mk.IIb Mod : Merlin XX 12 lb, Cy0_0/!!!1, CxMin1, squares, arm, trim                 OK clean

+Mosquito Mk.IV : Cy0_0/1, CxMin1, squares, arm
+Mosquito Mk.VI, Mk.XVIII : !!Merlin 25!!, Cy0_0/1, CxMin1, squares, arm, trim                  OK clean

+Spitfire Mk.V F 9 lb : Merlin 45, Cy0_0/!!!1, CxMin1, squares, arm, trim                       OK clean
+Spitfire Mk.V F 12 lb : Merlin 4512lb, Cy0_0/!!!1, CxMin1, squares, arm, trim                  OK clean
+Spitfire Mk.V F 12 lb trop 2H,4H : Merlin 45 12lb, Cy0_0/!!!1, CxMin1, squares, arm, trim      OK clean
+Spitfire Mk.V F 16 lb trop 2H : Merlin 45 16lb, Cy0_0/!!!1, CxMin1, squares, arm, trim         OK clean
+Spitfire Mk.V F 16 lb : Merlin 45 16lb, Cy0_0/!!!1, CxMin1, squares, arm, trim                 OK clean
+Spitfire Mk.V F 16 lb CW : Merlin 45 16lb, Cy0_0/!!!1, CxMin1, squares, arm, trim              OK clean
+Spitfire Mk.V LF M45M : Merlin 45M, Cy0_0/!!!1, CxMin1, squares, arm, trim                     OK clean
+Spitfire Mk.V LF M45M CW : Merlin 45M, Cy0_0/!!!1, CxMin1, squares, arm, trim                  OK clean
+Spitfire Mk.V HF M46 : Merlin 46 16lb, Cy0_0/!!!1, CxMin1, squares, arm, trim                  OK clean

+Spitfire Mk.VIII LF : Merlin 66Auto, Cy0_0/!!!1, CxMin1, squares, arm, trim                    OK clean
+Spitfire Mk.VIII LF CW : Merlin 66Auto, Cy0_0/!!!1, CxMin1, squares, arm, trim                 OK clean

+Spitfire Mk.IXc F M61 : Merlin 61, Cy0_0/!!!1, CxMin1, squares, arm, trim                      OK clean
+Spitfire Mk.IXc F M63 : Merlin 61, Cy0_0/!!!1, CxMin1, squares, arm, trim                      OK clean
+Spitfire Mk.IXc HF : Merlin 70, Cy0_0/!!!1, CxMin1, squares, arm, trim                         OK clean
+Spitfire Mk.IXc LF : Merlin 66, Cy0_0/!!!1, CxMin1, squares, arm, trim                         OK clean
+Spitfire Mk.IXc LF CW : Merlin 66, Cy0_0/!!!1, CxMin1, squares, arm, trim                      OK clean
+Spitfire Mk.IXc LF 25lb : Merlin 66 25lb, Cy0_0/!!!1, CxMin1, squares, arm, trim               OK clean
+Spitfire Mk.IXe HF : Merlin 70 Auto, Cy0_0/!!!1, CxMin1, squares, arm, trim                    OK clean
+Spitfire Mk.IXe LF CW : Merlin 66 Auto, Cy0_0/!!!1, CxMin1, squares, arm, trim                 OK clean
+Spitfire Mk.IXe LF CW 25lb : Merlin 66 25lb Auto, Cy0_0/!!!1, CxMin1, squares, arm, trim       OK clean

+Swordfish Mk.I : Cy0_0/1                                                                       OK clean

+Tempest Mk.V : Sabre IIA, Cy0_0/1, CxMin1, squares, arm, trim                                  OK clean
______________________________________________________________________________________________________________

USAAF


+A-20C,G : R-2600-23, Cy0_0/1, CxMin0/1 (Vmax=480km/h, VmaxH=515km/h @4000m), squares, arm, trim      OK clean

+B-17D,E,F,G : Cy0_0

+B-24D : !!!R-1830-65 (Changed boost to compressor stages (21), FTH, PropD, )!!!, Cy0_0/1(old Cxmin1 too high : caused lift bug), CxMin0/1, AOACritH_1 squares,arm   OK clean
+B-24J : Cy0_0/1

+B-25C,G,H : CxMin0/1, Cy0_0/1
+B-25J : R-2600-13, Cy0_0/1, CxMin0/1 (Vmax=432km/h, VmaxH=472km/h @4000m),  squares, arm, trim       OK clean

+B-29 : CxMin0, Cy0_0

+CW-21B : R-1820G5CW, Cy0_0/1, CxMin0/1, squares, arm, trim,                                          OK clean

+P-36A,A3 : R-1830-CSG (C3S1G), Cy0_0/1, CxMin0/1, squares, arm, trim                                 OK clean
+P-36A4, Mk.IV : R-1820-205, Cy0_0/1, CxMin0/1, squares, arm, trim                                    OK clean

+P-38J,L : V-1710-89,-91,-111,-113, Cy0_0/1, CxMin1, squares, arm, trim                               OK clean

+P-39D1,D2,P-400 : V-1710-35,-63, Cy0_0/1, CxMin1, squares, arm, trim                                 OK clean
+P-39N,Q1,Q21 : V-1710-85, Cy0_0/1, CxMin1, squares, arm, trim                                        OK clean

+P-40B,C : V-1710-33, Cy0_0/1, CxMin1, squares, arm, trim                                             OK clean
+P-40E : V-1710-39, M-105PA, Cy0_0/1, CxMin0/1, squares, arm, trim                                    OK clean
+P-40M : V-1710-81, Cy0_0/1, CxMin0/1, squares, arm, trim                                             OK clean

+P-47D-10,-22 :R-2800DoubleWasp, Cy0_0/1, CxMin1, squares, arm, trim                                  OK clean
+P-47D-27 : R-2800-59_THRU-40, Cy0_0/1, CxMin1, squares, arm, trim                                    OK clean
+P-47D-27 Late : R-2800-59_THRU-40_overboost, Cy0_0/1, CxMin1, squares, arm, trim                     OK clean

+P-51B,C : V-1650-3, Cy0_0/1, CxMin1, squares, arm, trim                                              OK clean
+Mustang III : V-1650-9, Cy0_0/1, CxMin1, squares, arm, trim                                          OK clean
+P-51D : V-1650-7, Cy0_0/1, CxMin1, squares, arm, trim                                                OK clean

+P-63 : V-1710-117, Cy0_0/1, CxMin1, squares, arm, trim                                               OK clean

^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
Refaire le Cy0_0/1

______________________________________________________________________________________________________________

Regia Aeronautica

+CR.42 : Cx, Cy0, fiat A.74 R1C38, squares, arm, trim, fuel+oil, (347 km/h S.L, 425 km/h @ 5300 m)    OK clean
+G.50 : Cxmin0/1, Cy0_0/1, fiat A.74 RC38, squares, arm, trim, (402 km/h SL, 470 km/h @ 5000 m)       OK clean
+MC.200 : fiat A.74 RC38, CxMin1, Cy0_0/1, fiat A.74 RC38, squares, arm, trim                         OK clean
+MC.202/205 : DB601A_MC, DB605B_MC, CxMin1, Cy0_0/1, fiat A.74 RC38, squares, arm, trim               OK clean          
+SM.79 : Alfa 126 RC34, Cy0_1, CxMin1, squares, arm, trim                                             OK clean
+Re.2000 : P.XI RC40, Cy0_0/1, CxMin1, squares, arm, trim                                             OK clean
______________________________________________________________________________________________________________

NL

+D.XXI DK, DU : Mercury VII, Cy0_0/1, CxMin0/1, squares, arm, trim                                    OK clean
+D.XXI serie 3 early, late : Mercury VII, Cy0_0/1, CxMin0/1, squares, arm, trim                       OK clean
______________________________________________________________________________________________________________

Pologne

+P-11c : Mercury VS2, Cy0_0/1, CxMin0, squares, arm, trim                                             OK clean
______________________________________________________________________________________________________________

Tchecoslovaquie

+B-534 : Avia_12Ydrs, Cy0_0/1, squares, arm, trim                                                     OK clean
______________________________________________________________________________________________________________

Yugoslavie

+IK-3 : Hispano-Suiza_12Y-29_Vee,CxMin1, Cy0_0/1, squares, arm, trim                                  OK clean
______________________________________________________________________________________________________________

Luftwaffe

+Ar-234 B-2 : Jumo004A, Wingspan, Length, Fuel, Oil, squares, arm, Cy0_1, CxMin1                      OK clean

+Bf-109 E-4,-4B,-7 : DB601A, Cy0_0/1, CxMin1, squares, arm, trim, Fuel, Oil                           OK clean
+Bf-109 E-7/Z : Man.Press indicator bugged can't mod engine properly, Cy0_0/1, CxMin1, squares, arm, trim    OK
+Bf-109 F-2 : DB601N, Empty weight, Cy0_0/1, CxMin1, squares, arm, trim, Fuel, Oil                    OK clean
+Bf-109 F-4 : DB601N_F4(E), Empty weight, Cy0_0/1, CxMin1, squares, arm, trim, Fuel, Oil              OK clean
+Bf-109 G-2 : DB605A, Empty weight, Cy0_0/1, CxMin1, squares, arm, trim, Fuel, Oil                    OK clean
+Bf-109 G-6 Early : DB605D to DB605A, Empty weight, Cy0_0/1, CxMin1, squares, arm, trim, Oil          OK clean
+Bf-109 G-6 Late : DB605D to DB605A, Empty weight, Cy0_0/1, CxMin1, squares, arm, trim, Oil           OK clean
+Bf-109 G-6 AS : DB605ASM, Empty weight, Cy0_0/1, CxMin1, squares, arm, trim, Oil                     OK clean
+Bf-109 G-10 : DB605DB, Empty weight, Cy0_0/1, CxMin1, squares, arm, trim, Oil                        OK clean
+Bf-109 G-14 : DB605AM, Empty weight, Cy0_0/1, CxMin1, squares, arm, trim, Oil                        OK clean
+Bf-109 K-4 : DB605DCM, Empty weight, Cy0_0/1, CxMin1, squares, arm, trim, Oil                        OK clean
+Bf-109 K-4-C4 : DB605DCM_C4, Empty weight, Cy0_0/1, CxMin1, squares, arm, trim, Oil                  OK clean

+Bf-110 C-4 : DB601A, Cy0_0/1, CxMin1, squares, arm, trim                                             OK clean
+Bf-110 C-4b : DB601N, Cy0_0/1, CxMin1, squares, arm, trim                                            OK clean
+Bf-110 D-1 : DB601A, Cy0_0/1, CxMin1, squares, arm, trim                                             OK clean
+Bf-110 E-2 : DB601N, Cy0_0/1, CxMin1, squares, arm, trim                                             OK clean
+Bf-110 F-2 : DB601F, Cy0_0/1, CxMin1, squares, arm, trim                                             OK clean
+Bf-110 G-2 : DB605B, Cy0_0/1, CxMin1, squares, arm, trim                                             OK clean

+Do-335 A-0 : DB603E, Cy0_1, CxMin1, squares, arm, trim, Empty weight                                 OK clean
+Do-335 V-13 : DB603E, Cy0_1, CxMin1, squares, arm, trim, Empty weight                                OK clean

+Fw-190 A-4/A-4FR : BMW801D-2, Cy0_0/1, CxMin1, squares, arm, trim, Length                            OK clean
+Fw-190 A-5 : BMW801D-2, Cy0_0/1, CxMin1, squares, arm, trim                                          OK clean
+Fw-190 A-5C-3: Cy0_0/1, CxMin1, squares, arm, trim                                                   OK clean
+Fw-190 A-6 : BMW801D-2, Cy0_0/1, CxMin1, squares, arm, trim                                          OK clean
+Fw-190 A-8 : BMW801D-2_165, Cy0_0/1, CxMin1, squares, arm, trim                                      OK clean
+Fw-190 A-9 : BMW801TS, Cy0_0/1, CxMin1, squares, arm, trim                                           OK clean
+Fw-190 A-9 Late : BMW801TS_182, Cy0_0/1, CxMin1, squares, arm, trim                                  OK clean
+Fw-190 F-8 : BMW801D-2_165, Cy0_0/1, CxMin1, squares, arm, trim                                      OK clean
+Fw-190 D-9 : Jumo213 A-1, Cy0_0/1, CxMin1, squares, arm, trim                                        OK clean
+Fw-190 D-9 Late : Jumo213 A-1 MW-50, Cy0_0/1, CxMin1, squares, arm, trim                             OK clean

+Ta-152 C : DB603L, Cy0_0/1, CxMin1, squares, arm                                                     OK clean
+Ta-152 H-1 : Jumo213 E-1 MW-50, Cy0_0/1, CxMin1, squares, arm                                        OK clean

+He-111 H-2 : Jumo211 A-3,  Cy0_1, CxMin0/1, squares, arm, trim, Empty weight                         OK clean
+He-111 H-6 : Jumo211 F-2,  Cy0_1, CxMin0/1, squares, arm, trim, Empty weight                         OK clean
+He-111 H-12 : Jumo211 F-2,  Cy0_1, CxMin0/1, squares, arm, trim, Empty weight                        OK clean
+He-111 H-16 : Jumo211 F-2,  Cy0_1, CxMin0/1, squares, arm, trim, Empty weight                        OK clean

+He-162 A-2 : Cy0_1, CxMin1, squares, arm                                                             OK clean

+He-177 A-3 : DB610, CxMin1, Cy0_0/1, squares, arm, trim, Empty weight                                OK clean

~Ho-229 : CxMin1, Cy0_0/1, squares, arm

+Hs-129 B-2 : Empty weight, Length, Gnome-Rhone 14M,  Cy0_0/1, CxMin0/1, squares, arm, trim           OK clean
+Hs-129 B-3 : Empty weight, Length, Gnome-Rhone 14M,  Cy0_0/1, CxMin0/1, squares, arm, trim           OK clean

+Ju-87 B-2 : Jumo211 D, Cy0_1, CxMin1, squares, arm, trim                                             OK clean
+Ju-87 D-3 : Jumo211 F-1_Ju(J-1), Cy0_1, CxMin1, squares, arm, trim                                   OK clean
+Ju-87 D-5 : Jumo211 F-1_Ju(J-1), Cy0_1, CxMin1, squares, arm, trim                                   OK clean
+Ju-87 G-1 : Jumo211 F-1_Ju(J-1), Cy0_1, CxMin1, squares, arm, trim                                   OK clean

+Ju-88 A-1 : Jumo211 G-1, CxMin0/1, Cy0_0/1                                                           OK clean
+Ju-88 A-4/Mistel/Torp : Jumo211 J-1, CxMin0/1, Cy0_0/1, squares, arm, trim                           OK clean
+Ju-88 A-5 : Jumo211 G-1, CxMin0/1, Cy0_0/1, squares, arm, trim                                       OK clean
+Ju-88 A-6 : Jumo211 G-1, CxMin0/1, Cy0_0/1                                                           OK clean
+Ju-88 A-17 : Jumo211 F-1 to J-1, CxMin0/1, Cy0_0/1, squares, arm, trim                               OK clean
+Ju-88 C-2 : Jumo211 G-1, CxMin0/1, Cy0_0/1                                                           OK clean
+Ju-88 P-1 : Jumo211 J-1, CxMin0/1, Cy0_0/1, squares, arm, trim                                       OK clean

+Me-163 B-1 : CxMin1, Cy0_0/1, squares, arm, trim                                                     OK clean

+Me-262 A-1a, A-1a/U-4 : CxMin1, Cy0_0/1, squares, arm                                                OK clean

~Ta-183 : CxMin1, Cy0_0/1, squares, arm
______________________________________________________________________________________________________________

Roumanie

+IAR 80, 81a : 14K 1000A, squares, arm, Cy0_1, Cxmin1, trim                                           OK clean